**Timer ZS 3**

Timer for automatic, time-dependent control of the fans.

Digital time switch with 24 hour switching program.

20 on and off switch settings are possible.

With automatic switching between summer and winter operation.

Shortest time which can be set 1 min.

Technical data

|  |  |
| --- | --- |
| Article: | ZS 3 |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 2 A |
| Degree of protection: | IP 40 |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,2 kg |
| Width: | 120 mm |
| Height: | 60 mm |
| Depth: | 35 mm |
| Width with packaging: | 130 mm |
| Height with packaging: | 40 mm |
| Depth with packaging: | 65 mm |
| Remote control: |  -  |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799577904 |
| Article number: | 0157.0790 |

Manufacturer: MAICO

ZS 3 Timer