**Sealing kit RLS G1V**

Sealing kit for the room air control of the WS 75 Powerbox.

The RLS G1 WS room air control can thus be installed in a flush-mounted box.

Technical data

|  |  |
| --- | --- |
| Article: | RLS G1V |
| Material: | Glass |
| Colour: | White |
| Weight: | 0,16 kg |
| Weight including packaging: | 0,26 kg |
| Width: | 130 mm |
| Height: | 92 mm |
| Depth: | 15 mm |
| Width with packaging: | 265 mm |
| Height with packaging: | 165 mm |
| Depth with packaging: | 49 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799992486 |
| Article number: | 0093.1591 |

Manufacturer: MAICO

RLS G1V Sealing kit