**Door contact switch TS 1**

Door contact switch as spare part for the WR 300, WR 400, WR 600, WS 150, WS 170 and WS 250 centralised ventilation units.

Door contact – n/o contact 16A.

Technical data

|  |  |
| --- | --- |
| Article: | TS 1 |
| Type of voltage: | Alternating current |
| Rated voltage: | 125 V - 250 V |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,05 kg |
| Width: | 30 mm |
| Height: | 40 mm |
| Depth: | 12 mm |
| Width with packaging: | 175 mm |
| Height with packaging: | 250 mm |
| Depth with packaging: | 20 mm |
| Range: | K |
| GTIN (EAN): | 4012799101444 |
| Article number: | E157.1150.0000 |

Manufacturer: MAICO

TS 1 Door contact switch