**Axial wall fan DZQ 45/6 A-Ex**

Technical data

|  |  |
| --- | --- |
| Article: | DZQ 45/6 A-Ex |
| Model: | Square wall plate |
| Air flow volume: | 4.300 m³/h |
| Rotating speed: | 960 1/min |
| Power consumption: | 200 W |
| Imax: | 0,64 A |
| Weight: | 16,3 |
| IA/IN: | 2,7 |
| Certified as explosion proof: | 84/3896 |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799837800 |
| Article number: | 0083.0780 |

Manufacturer: MAICO

DZQ 45/6 A-Ex Axial wall fan