**Backflow preventer set WS 75 RK-Set**

The backflow preventers minimize the ingress of air and external noise when the unit is switched off.

Set consists of 2 backflow preventers.

Technical data

|  |  |
| --- | --- |
| Article: | WS 75 RK-Set |
| Housing material: | Synthetic material |
| Colour: | Black |
| Weight: | 0,14 kg |
| Weight including packaging: | 0,15 kg |
| Width: | 170 mm |
| Height: | 84 mm |
| Depth: | 80 mm |
| Width with packaging: | 267 mm |
| Height with packaging: | 156 mm |
| Depth with packaging: | 100 mm |
| Packing unit: | 1 set (2 pieces) |
| Range: | K |
| GTIN (EAN): | 4012799992448 |
| Article number: | 0093.1587 |

Manufacturer: MAICO

WS 75 RK-Set Backflow preventer set