**Shutter, pull device VD 30-Ex**

Airstream operated shutters with pull device for manual operation.

Can be used only in rooms up to 5 m high due to thermal convection.

Up to DN 400 nominal size: Shutter opens from 930 min-1 onwards.

Up to DN 500 nominal size: Shutter opens from 715 min-1 onwards.

Technical data

|  |  |
| --- | --- |
| Article: | VD 30-Ex |
| Weight: | 3 |
| Type of shutter: | Airstream-operated opening/closing |
| Suitable for nominal size: | 300 mm |
| Explosion protection: | Ex II 2G |
| Ex version: | antistatic |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799936329 |
| Article number: | 0093.0632 |

Manufacturer: MAICO

VD 30-Ex Shutter, pull device