**Mounting clamp MT-LS125**

Two-part mounting clamp with pre-fitted clamping screws for installing the thermally insulated MAICOTherm MT ventilation duct system.

Fitted with swivel screw for safe and simple quick-coupling mounting.

Quick installation because the ducts/elbows can be fitted without any tools.

Technical data

|  |  |
| --- | --- |
| Article: | MT-LS125 |
| Air direction: | Ventilation and air extraction |
| Installation site: | Ceiling / Wall / Floor |
| Material: | Sheet steel, galvanised |
| Weight: | 0,16 kg |
| Weight including packaging: | 0,2 kg |
| Nominal size: | 125 mm |
| Suitable for nominal size: | 160 mm |
| Width: | 215 mm |
| Height: | 135 mm |
| Depth: | 20 mm |
| Width with packaging: | 215 mm |
| Height with packaging: | 135 mm |
| Depth with packaging: | 20 mm |
| Thread: | M8 |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799180654 |
| Article number: | 0018.0065 |

Manufacturer: MAICO

MT-LS125 Mounting clamp