**Bypass for heat exchanger SK 300 WT**

Bypass for WT 300 for winter or summer operation.

With symbol identification for summer and winter operation.

Reversible adaptor.

Technical data

|  |  |
| --- | --- |
| Article: | SK 300 WT |
| Installation position: | vertical / horizontal |
| Material: | EPS |
| Weight: | 0,7 kg |
| Weight including packaging: | 0,7 kg |
| Width: | 720 mm |
| Height: | 320 mm |
| Depth: | 110 mm |
| Width with packaging: | 720 mm |
| Height with packaging: | 320 mm |
| Depth with packaging: | 110 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799520511 |
| Article number: | 0152.0051 |

Manufacturer: MAICO

SK 300 WT Bypass for heat exchanger