**Housing GH AP ER 60/100 F**

Housing with cover, filter and time strip as spare part for ER-AP 60 F, ER-APB 60 F, ER-AP 100 F and ER-APB 100 F surface-mounted fans.

For model with light control.

Technical data

|  |  |
| --- | --- |
| Article: | GH AP ER 60/100 F |
| Housing material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,56 kg |
| Weight including packaging: | 0,78 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Width: | 230 mm |
| Height: | 145 mm |
| Depth: | 230 mm |
| Width with packaging: | 270 mm |
| Height with packaging: | 155 mm |
| Depth with packaging: | 280 mm |
| Range: | B |
| GTIN (EAN): | 4012799100201 |
| Article number: | E059.1036.9101 |

Manufacturer: MAICO

GH AP ER 60/100 F Housing