**Folded spiral-seams duct WFR 125**

Folded spiral-seams ducts for ventilation systems in controlled domestic ventilation

Technical data

|  |  |
| --- | --- |
| Article: | WFR 125 |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel, galvanised |
| Nominal size: | 125 mm |
| Length: | 3 m |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799550778 |
| Article number: | 0055.0077 |

Manufacturer: MAICO

WFR 125 Folded spiral-seams duct