**Intermediate piece, asymmetric USAN80/200/125**

Features

Round to square transition piece.

Square: Sleeve size.

Round (asymmetrical): Nipple size.

Surface: Sendzimir galvanised.

Suitable for connection with MF-WE slide-in adaptor.

Technical data

|  |  |
| --- | --- |
| Article: | USAN80/200/125 |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel, Sendzimir galvanised |
| Weight: | 0,58 kg |
| Weight including packaging: | 0,58 kg |
| Nominal size: | 125 mm |
| Channel dimension: | 200 mm x Array x 80 mm |
| Width: | 200 mm |
| Height: | 200 mm |
| Depth: | 130 mm |
| Width with packaging: | 200 mm |
| Height with packaging: | 200 mm |
| Depth with packaging: | 130 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799556725 |
| Article number: | 0055.0672 |

Manufacturer: MAICO

USAN80/200/125 Intermediate piece, asymmetric