**45° channel elbows, vertical KB45V/55/220**

Features

Vertical channel elbow, collar size. Surface: Sendzimir galvanised.

Technical data

|  |  |
| --- | --- |
| Article: | KB45V/55/220 |
| Material: | Sheet steel, Sendzimir galvanised |
| Channel dimension: | 220 mm x Array x 55 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799556015 |
| Article number: | 0055.0601 |

Manufacturer: MAICO

KB45V/55/220 45° channel elbows, vertical