**Axial duct fan DZR 50/6 A-Ex**

Technical data

|  |  |
| --- | --- |
| Article: | DZR 50/6 A-Ex |
| Air flow volume: | 5.800 m³/h |
| Rotating speed: | 920 1/min |
| Nominal output: | 175 W |
| Inom: | 0,71 A |
| Imax: | 0,71 A |
| Weight: | 20,1 |
| IA/IN: | 2,2 |
| Certified as explosion proof: | 84/3898 |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799867852 |
| Article number: | 0086.0785 |

Manufacturer: MAICO

DZR 50/6 A-Ex Axial duct fan