**Mounting support UPM 60/100**

Mounting support for installation of ER-GH and ER-UP.. recess-mounted housing on walls, ceilings or in shafts.

With slots for precise adjustment of the fan housing.

Packing unit:

2 L-shaped angle plates

4 mounting screws.

Technical data

|  |  |
| --- | --- |
| Article: | UPM 60/100 |
| Material: | Sheet steel, galvanised |
| Weight: | 0,46 kg |
| Weight including packaging: | 0,5 kg |
| Width: | 40 mm |
| Height: | 350 mm |
| Depth: | 50 mm |
| Width with packaging: | 40 mm |
| Height with packaging: | 350 mm |
| Depth with packaging: | 50 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799180104 |
| Article number: | 0018.0010 |

Manufacturer: MAICO

UPM 60/100 Mounting support