**Air filter, replacement ZF 17 S**

ZF 17 S: Replacement air filter for ER 17/60-2... and ER 17/100... fan insert.

Technical data

|  |  |
| --- | --- |
| Article: | ZF 17 S |
| Installation position: | vertical / horizontal |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,02 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Width: | 220 mm |
| Height: | 34 mm |
| Depth: | 175 mm |
| Width with packaging: | 260 mm |
| Height with packaging: | 175 mm |
| Depth with packaging: | 20 mm |
| Packing unit: | 5 pieces |
| Range: | B |
| GTIN (EAN): | 4012799936756 |
| Article number: | 0093.0675 |

Manufacturer: MAICO

ZF 17 S Air filter, replacement