**Shell kit PP 60 KL-SR**

Features

Shell kit for fitting in the window soffit.

Scope of delivery:

PVC wall sleeve with two plaster protective covers and eight shims for aligning sleeve in wall hole.

Aluminium/stainless steel soffit element.

Is needed as accessory for PP 60 K-SE final assembly set.

Technical data

|  |  |
| --- | --- |
| Article: | PP 60 KL-SR |
| Air flow volume: | 17 m³/h / 21 m³/h / 27 m³/h / 39 m³/h / 46 m³/h |
| Installation site: | Window soffit |
| Installation position: | horizontal |
| Material: | Aluminium/stainless steel |
| Colour: | Stainless steel, brushed |
| Weight: | 2,7 kg |
| Weight including packaging: | 4,276 kg |
| Nominal size: | 200 mm |
| Width: | 670 mm |
| Height: | 360 mm |
| Depth: | 574 mm |
| Width with packaging: | 690 mm |
| Height with packaging: | 320 mm |
| Depth with packaging: | 400 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799952060 |
| Article number: | 0095.0206 |

Manufacturer: MAICO

PP 60 KL-SR Shell kit