**Shell kit PP 60 KA-SRW**

Shell kit for fitting in the external wall.

Scope of delivery:

PVC wall sleeve with two plaster protective covers and eight shims for aligning sleeve in wall hole.

External cover made from galvanised sheet steel, white similar to RAL 9010.

Is needed as an accessory for the PP 60 K-SE final assembly kit.

Technical data

|  |  |
| --- | --- |
| Article: | PP 60 KA-SRW |
| Air flow volume: | 17 m³/h / 22 m³/h / 30 m³/h / 41 m³/h / 50 m³/h |
| Installation site: | Outside wall |
| Installation position: | horizontal |
| Material: | Sheet steel, galvanised |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 2,2 kg |
| Weight including packaging: | 3,052 kg |
| Nominal size: | 200 mm |
| Width: | 545 mm |
| Height: | 286 mm |
| Depth: | 250 mm |
| Width with packaging: | 280 mm |
| Height with packaging: | 280 mm |
| Depth with packaging: | 510 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799952152 |
| Article number: | 0095.0215 |

Manufacturer: MAICO

PP 60 KA-SRW Shell kit