**Vibration damper GPI 10-20**

4 vibration dampers for the vibration-damped mounting of fans.

The load capacity refers to a vibration damper.

Technical data

|  |  |
| --- | --- |
| Article: | GPI 10-20 |
| Material: | Steel/plastic |
| Colour: | Black |
| Weight: | 0,02 kg |
| Weight including packaging: | 0,02 kg |
| Maximum working load: | 20 kg |
| Minimum working load: | 10 kg |
| Width: | 20 mm |
| Height: | 15 mm |
| Depth: | 20 mm |
| Width with packaging: | 20 mm |
| Height with packaging: | 15 mm |
| Depth with packaging: | 20 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799732730 |
| Article number: | 0073.0273 |

Manufacturer: MAICO

GPI 10-20 Vibration damper